LED/text message/email alert of change in temperature

Internal temperature of equipment the device is attached to

ESP32 Microcontroller controls data from temp sensor

User setup of device via Bluetooth

Input Controller Actuator Output

Temperature Sensor on device

 Sensor